WeOS Power Ethernet MIB Conformance
====================================

MIB:     Power Ethernet MIB (RFC 3621)

Supported Object Groups
=======================
pethPsePortGroup
pethMainPseGroup
pethMainPowerNotificationGroup

Variations
==========
pethPsePortGroup
- pethPsePortGroupIndex
  ACCESS: read-only
- pethPsePortIndex
  ACCESS: read-only
- pethPsePortAdminEnable
  ACCESS: read-only
- pethPsePortPowerPairsControlAbility
  ACCESS: read-only
- pethPsePortPowerPairs
  ACCESS: read-only
- pethPsePortPowerPriority
  ACCESS: read-only
- pethPsePortMPSAbsentCounter
  ACCESS: not-implemented
- pethPsePortInvalidSignatureCounter
  ACCESS: not-implemented
- pethPsePortPowerDeniedCounter
  ACCESS: not-implemented
- pethPsePortOverLoadCounter
  ACCESS: not-implemented
- pethPsePortShortCounter
  ACCESS: not-implemented
- pethPsePortType
  ACCESS: read-only
  DESCRIPTION: "Displays the port name."
pethMainPseGroup
- pethMainPseGroupIndex
  ACCESS: read-only
- pethMainPseUsageThreshold
  ACCESS: not-implemented
pethMainPowerNotificationGroup
- pethPsePortOnOffNotification
  ACCESS: not-implemented
