WeOS IF MIB Conformance
=======================

MIB:     IF MIB
Version: "200006140000Z"

Supported Object Groups
=======================
ifGeneralInformationGroup
ifFixedLengthGroup
ifHCFixedLengthGroup
ifPacketGroup
ifHCPacketGroup
ifVHCPacketGroup
ifRcvAddressGroup
linkUpDownNotificationsGroup

Variations
==========
ifGeneralInformationGroup
- ifAdminStatus
  DESCRIPTION: Unable to set testing(3). Reading testing(3) means that
  the interface is forced up and link propagation disabled.
- ifOperStatus
  SYNTAX: INTEGER { up(1), down(2) }
- ifLastChange
  ACCESS: read-only
  DESCRIPTION: The value of sysUpTime at the time the interface entered
  its current operational state
- ifLinkUpDownTrapEnable
  ACCESS: read-write access only available for physical ports.
- ifAlias
  ACCESS: read-only
- ifTableLastChange
  ACCESS: not-implemented
ifPacketGroup
- ifOutMulticastPkts
  DESCRIPTION: Only available for physical ports.
- ifOutBroadcastPkts
  DESCRIPTION: Only available for physical ports.
- ifPromiscuousMode
  ACCESS: read-only
ifHCPacketGroup
- ifOutMulticastPkts
  DESCRIPTION: Only available for physical ports.
- ifOutBroadcastPkts
  DESCRIPTION: Only available for physical ports.
- ifPromiscuousMode
  ACCESS: read-only
ifVHCPacketGroup
- ifHCOutMulticastPkts
  DESCRIPTION: Only available for physical ports.
- ifHCOutBroadcastPkts
  DESCRIPTION: Only available for physical ports.
- ifOutMulticastPkts
  DESCRIPTION: Only available for physical ports.
- ifOutBroadcastPkts
  DESCRIPTION: Only available for physical ports.
- ifPromiscuousMode
  ACCESS: read-only
ifRcvAddressGroup
- ifRcvAddressStatus
  ACCESS: read-only
- ifRcvAddressType
  ACCESS: read-only
