WeOS LAG MIB Conformance
========================

MIB:     LAG MIB (IEEE 802.1AX-2014)
Version: "201412180000Z"

Supported Object Groups
=======================
dot3adAggGroup
dot3adAggPortListGroup
dot3adAggPortGroup

Variations
==========
dot3adAggGroup
- dot3adAggActorSystemPriority:
  ACCESS: read-only
- dot3adAggActorSystemID:
  ACCESS: read-only
- dot3adAggAggregateOrIndividual
  DESCRIPTION: Only aggregates are listed in table (no individual links).
- dot3adAggActorAdminKey:
  ACCESS: not-implemented
- dot3adAggActorOperKey:
  ACCESS: not-implemented
- dot3adAggCollectorMaxDelay:
  ACCESS: not-implemented
dot3adAggPortGroup
- dot3adAggPortActorSystemPriority:
  ACCESS: read-only
- dot3adAggPortActorAdminKey:
  ACCESS: read-only
- dot3adAggPortActorOperKey
  ACCESS: not-implemented
- dot3adAggPortPartnerAdminSystemPriority:
  ACCESS: not-implemented
- dot3adAggPortPartnerAdminSystemID:
  ACCESS: not-implemented
- dot3adAggPortPartnerAdminKey:
  ACCESS: not-implemented
- dot3adAggPortActorPortPriority:
  ACCESS: read-only
- dot3adAggPortPartnerAdminPort:
  ACCESS: not-implemented
- dot3adAggPortPartnerAdminPortPriority:
  ACCESS: not-implemented
- dot3adAggPortActorAdminState:
  ACCESS: not-implemented
- dot3adAggPortPartnerAdminState:
  ACCESS: not-implemented
- dot3adAggPortAggregateOrIndividual
  DESCRIPTION: Only ports being member of an aggregate are listed in table (no individual ports).
